interface TenGigabitEthernet1/16

description TUNO-OLT-UF-8PX1

switchport trunk native vlan 99

switchport mode trunk

mtu 9198

no channel-group 4 mode active

end

interface Port-channel4

description TO-CCSC4500TFINX1

switchport

switchport trunk native vlan 99

switchport mode trunk

mtu 9198

end

########################################

1809 3250 TUNO-CLUB-PTO-AZUL

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3250

description CLUB-PTO-AZUL;ID:26302

bandwidth 51200

encapsulation dot1Q 3250

ip address 172.23.243.37 255.255.255.252

ipv6 address 2803:D480:0:61::8053/64

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.245.0 255.255.255.252 172.23.243.38 name GPON-VL3250-TUNO-CLUB-PTO-AZUL

ipv6 route 2803:D480:3:100::/56 2803:D480:0:61::2 name GPON-VL3250-TUNO-CLUB-PTO-AZUL

interface TenGigabitEthernet0/1/0.1809

description CLUB-PTO-AZUL;ID:26302

bandwidth 51200

encapsulation dot1Q 1809

ip address 172.23.243.37 255.255.255.252

ipv6 address 2803:D480:0:61::8053/64

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.245.0 255.255.255.252 172.23.243.38 name GPON-VL1809-TUNO-CLUB-PTO-AZUL

ipv6 route 2803:D480:3:100::/56 2803:D480:0:61::2 name GPON-VL1809-TUNO-CLUB-PTO-AZUL

----------------CCSJ4500CREX2------------

ssh [soporte2@172.23.253.59](mailto:soporte2@172.23.253.59)

set vlan TUNO-CLUB-PTO-AZUL vlan-id 1809

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-CLUB-PTO-AZUL

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-CLUB-PTO-AZUL

----------------CCSC4500TUNOX1------------

ssh [soporte2@172.23.253.](mailto:soporte2@172.23.253.)20

vlan 1809

name TUNO-CLUB-PTO-AZUL

interface po4

switchport trunk allowed vlan add 1809

########################################

1810 3251 TUNO-ESP-ORIENTALES

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3251

description ESP-ORIENTALES;ID:26287

bandwidth 51200

encapsulation dot1Q 3251

ip address 172.23.243.41 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.252.112 255.255.255.252 172.23.243.42 name GPON-VL3251-TUNO-ESP-ORIENTALES

interface TenGigabitEthernet0/1/0.1810

description ESP-ORIENTALES;ID:26287

bandwidth 51200

encapsulation dot1Q 1810

ip address 172.23.243.41 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.252.112 255.255.255.252 172.23.243.42 name GPON-VL1810-TUNO-ESP-ORIENTALES

----------------CCSJ4500CREX2------------

ssh [soporte2@172.23.253.59](mailto:soporte2@172.23.253.59)

set vlan TUNO-ESP-ORIENTALES vlan-id 1810

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-ESP-ORIENTALES

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-ESP-ORIENTALES

----------------CCSC4500TUNOX1------------

ssh [soporte2@172.23.253.](mailto:soporte2@172.23.253.)20

vlan 1810

name TUNO-ESP-ORIENTALES

interface po4

switchport trunk allowed vlan add 1810

########################################

1811 3252 TUNO-COPIKON

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3252

description TUNO-COPIKON

bandwidth 51200

encapsulation dot1Q 3252

ip address 172.23.243.45 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.245.4 255.255.255.252 172.23.243.46 name GPON-VL3252-TUNO-COPIKON

interface TenGigabitEthernet0/1/0.1811

description COPIKON;ID:

bandwidth 51200

encapsulation dot1Q 1811

ip address 172.23.243.45 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.245.4 255.255.255.252 172.23.243.46 name GPON-VL1811-TUNO-COPIKON

----------------CCSJ4500CREX2------------

ssh [soporte2@172.23.253.59](mailto:soporte2@172.23.253.59)

set vlan TUNO-COPIKON vlan-id 1811

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-COPIKON

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-COPIKON

----------------CCSC4500TUNOX1------------

ssh [soporte2@172.23.253.](mailto:soporte2@172.23.253.)20

vlan 1811

name TUNO-COPIKON

interface po4

switchport trunk allowed vlan add 1811

########################################

|  |  |  |
| --- | --- | --- |
| 1812 | 3253 | TUNO-LOCATEL-SM |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3253

description LOCATEL-SM;ID:25929

bandwidth 71680

encapsulation dot1Q 3253

ip address 172.23.253.101 255.255.255.252

service-policy input 70M

service-policy output 70M

exit

ip route 181.225.48.216 255.255.255.248 172.23.253.102 name GPON-VL3253-TUNO-LOCATEL-SM

interface TenGigabitEthernet0/1/0.1812

description LOCATEL-SM;ID:25929

bandwidth 71680

encapsulation dot1Q 1812

ip address 172.23.253.101 255.255.255.252

service-policy input 70M

service-policy output 70M

exit

ip route 181.225.48.216 255.255.255.248 172.23.253.102 name GPON-VL1812-TUNO-LOCATEL-SM

----------------CCSJ4500CREX2------------

ssh [soporte2@172.23.253.59](mailto:soporte2@172.23.253.59)

set vlan TUNO-LOCATEL-SM vlan-id 1812

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-LOCATEL-SM

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-LOCATEL-SM

----------------CCSC4500TUNOX1------------

ssh [soporte2@172.23.253.](mailto:soporte2@172.23.253.)20

vlan 1812

name TUNO-LOCATEL-SM

interface po4

switchport trunk allowed vlan add 1812

########################################

1813 3258 TUNO-CORP-CALL-77

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3258

description TUNO-CORP-CALL-77

bandwidth 102400

encapsulation dot1Q 3258

ip address 172.23.243.141 255.255.255.252

service-policy input 100M

service-policy output 100M

exit

ip route 190.94.199.140 255.255.255.252 172.23.243.142 name GPON-VL3258-TUNO-CORP-CALL-77

interface TenGigabitEthernet0/1/0.1813

description CORP-CALL-77;ID:

bandwidth 102400

encapsulation dot1Q 1813

ip address 172.23.243.141 255.255.255.252

service-policy input 100M

service-policy output 100M

exit

ip route 190.94.199.140 255.255.255.252 172.23.243.142 name GPON-VL813-TUNO-CORP-CALL-77

----------------CCSJ4500CREX2------------

ssh [soporte2@172.23.253.59](mailto:soporte2@172.23.253.59)

set vlan TUNO-CORP-CALL-77 vlan-id 1813

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-CORP-CALL-77

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-CORP-CALL-77

----------------CCSC4500TUNOX1------------

ssh [soporte2@172.23.253.](mailto:soporte2@172.23.253.)20

vlan 1813

name TUNO-CORP-CALL-77

interface po4

switchport trunk allowed vlan add 1813

########################################

1814 3259 TUNO-EXCLU-VAGU

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3259

description TUNO-EXCLU-VAGU

bandwidth 102400

encapsulation dot1Q 3259

ip address 172.23.241.173 255.255.255.252

service-policy input 100M

service-policy output 100M

exit

ip route 190.94.244.120 255.255.255.252 172.23.241.174 name GPON-VL3259-TUNO-EXCLU-VAGU

interface TenGigabitEthernet0/1/0.1814

description EXCLU-VAGU;ID:

bandwidth 102400

encapsulation dot1Q 1814

ip address 172.23.241.173 255.255.255.252

service-policy input 100M

service-policy output 100M

exit

ip route 190.94.244.120 255.255.255.252 172.23.241.174 name GPON-VL1814-TUNO-EXCLU-VAGU

----------------CCSJ4500CREX2------------

ssh [soporte2@172.23.253.59](mailto:soporte2@172.23.253.59)

set vlan TUNO-EXCLU-VAGU vlan-id 1814

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-EXCLU-VAGU

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-EXCLU-VAGU

----------------CCSC4500TUNOX1------------

ssh [soporte2@172.23.253.](mailto:soporte2@172.23.253.)20

vlan 1814

name TUNO-EXCLU-VAGU

interface po4

switchport trunk allowed vlan add 1814

########################################

1815 3260 TUNO-REINALDO

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3260

description TUNO-REINALDO;ID:4

bandwidth 102400

encapsulation dot1Q 3260

ip address 190.94.199.45 255.255.255.252

service-policy input 100M

service-policy output 100M

interface TenGigabitEthernet0/1/0.1815

description TUNO-REINALDO;ID:4

bandwidth 102400

encapsulation dot1Q 1815

ip address 190.94.199.45 255.255.255.252

service-policy input 100M

service-policy output 100M

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-REINALDO vlan-id 1815

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-REINALDO

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-REINALDO

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1815

name TUNO-REINALDO

interface po4

switchport trunk allowed vlan add 1815

########################################

1816 3261 TUNO-MDA-TV

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3261

description TUNO-MDA-TV

bandwidth 61440

encapsulation dot1Q 3261

ip address 172.23.243.93 255.255.255.252

service-policy input 60M

service-policy output 60M

exit

ip route 190.94.244.16 255.255.255.252 172.23.243.94 name GPON-VL3261-TUNO-MDA-TV

interface TenGigabitEthernet0/1/0.1816

description TUNO-MDA-TV;ID:

bandwidth 61440

encapsulation dot1Q 1816

ip address 172.23.243.93 255.255.255.252

service-policy input 60M

service-policy output 60M

exit

ip route 190.94.244.16 255.255.255.252 172.23.243.94 name GPON-VL1816-TUNO-MDA-TV

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-MDA-TV vlan-id 1816

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-MDA-TV

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-MDA-TV

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1816

name TUNO-MDA-TV

interface po4

switchport trunk allowed vlan add 1816

########################################

1817 3262 TUNO-ASA-STEKI

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3262

description TUNO-ASA-STEKI

bandwidth 51200

encapsulation dot1Q 3262

ip address 172.23.244.241 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.250.224 255.255.255.252 172.23.244.242 name GPON-VL362-TUNO-ASA-STEKI

interface TenGigabitEthernet0/1/0.1817

description ASA-STEKI;ID:

bandwidth 51200

encapsulation dot1Q 1817

ip address 172.23.244.241 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.250.224 255.255.255.252 172.23.244.242 name GPON-VL1817-TUNO-ASA-STEKI

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-ASA-STEKI vlan-id 1817

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-ASA-STEKI

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-ASA-STEKI

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1817

name TUNO-ASA-STEKI

interface po4

switchport trunk allowed vlan add 1817

########################################

1818 3263 TUNO-SKYTEX

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3263

description SKYTEX;ID:26049

bandwidth 51200

encapsulation dot1Q 3263

ip address 172.23.244.249 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.199.192 255.255.255.252 172.23.244.250 name GPON-VL3263-TUNO-SKYTEX

interface TenGigabitEthernet0/1/0.1818

description SKYTEX;ID:26049

bandwidth 51200

encapsulation dot1Q 1818

ip address 172.23.244.249 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.199.192 255.255.255.252 172.23.244.250 name GPON-VL1818-TUNO-SKYTEX

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-SKYTEX vlan-id 1818

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-SKYTEX

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-SKYTEX

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1818

name TUNO-SKYTEX

interface po4

switchport trunk allowed vlan add 1818

########################################

1819 3264 TUNO-SKYTEX-2

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3264

description SKYTEX-2;ID:26049

bandwidth 51200

encapsulation dot1Q 3264

ip address 172.23.244.61 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.199.196 255.255.255.252 172.23.244.62 name TUNO-SKYTEX-2

interface TenGigabitEthernet0/1/0.1819

description SKYTEX-2;ID:26049

bandwidth 51200

encapsulation dot1Q 1819

ip address 172.23.244.61 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.199.196 255.255.255.252 172.23.244.62 name GPON-VL1819-TUNO-SKYTEX-2

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-SKYTEX-2 vlan-id 1819

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-SKYTEX-2

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-SKYTEX-2

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1819

name TUNO-SKYTEX-2

interface po4

switchport trunk allowed vlan add 1819

########################################

1820 3265 TUNO-PRODEC

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3265

description PRODEC;ID:26240

bandwidth 51200

encapsulation dot1Q 3265

ip address 172.23.243.173 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.244.64 255.255.255.252 172.23.243.174 name GPON-VL3265-TUNO-SKYTEX

interface TenGigabitEthernet0/1/0.1820

description PRODEC;ID:26240

bandwidth 51200

encapsulation dot1Q 1820

ip address 172.23.243.173 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.244.64 255.255.255.252 172.23.243.174 name GPON-VL1820-TUNO-PRODEC

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-PRODEC vlan-id 1820

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-PRODEC

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-PRODEC

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1820

name TUNO-PRODEC

interface po4

switchport trunk allowed vlan add 1820

########################################

1821 3266 TUNO-MOBRITECK-IMP

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3266

description TUNO-MOBRITECK-IMP

bandwidth 40960

encapsulation dot1Q 3266

ip address 172.23.243.189 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.244.96 255.255.255.252 172.23.243.190 name RED1-TUNO-MOBRITECK-IMP

interface TenGigabitEthernet0/1/0.1821

description MOBRITECK-IMP;ID:

bandwidth 40960

encapsulation dot1Q 1821

ip address 172.23.243.189 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.244.96 255.255.255.252 172.23.243.190 name GPON-VL1821-TUNO-MOBRITECK-IMP

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-MOBRITECK-IMP vlan-id 1821

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-MOBRITECK-IMP

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-MOBRITECK-IMP

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1821

name TUNO-MOBRITECK-IMP

interface po4

switchport trunk allowed vlan add 1821

########################################

1822 3267 TUNO-WORLD-TRADING

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3267

description WORLD-TRADING;ID:26211

bandwidth 40960

encapsulation dot1Q 3267

ip address 172.23.254.85 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.208.28 255.255.255.252 172.23.254.86 name RED1-VL3267-TUNO-WORLD-TRADING

ip route 190.94.251.128 255.255.255.248 172.23.254.86 name RED1-VL3267-TUNO-WORLD-TRADING

interface TenGigabitEthernet0/1/0.1822

description WORLD-TRADING;ID:26211

bandwidth 40960

encapsulation dot1Q 1822

ip address 172.23.254.85 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.208.28 255.255.255.252 172.23.254.86 name GPON-VL1822-TUNO-WORLD-TRADING

ip route 190.94.251.128 255.255.255.248 172.23.254.86 name RED1-VL1822-TUNO-WORLD-TRADING

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-WORLD-TRADING vlan-id 1822

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-WORLD-TRADING

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-WORLD-TRADING

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1822

name TUNO-WORLD-TRADING

interface po4

switchport trunk allowed vlan add 1822

########################################

1823 3268 TUNO-TOP-FOOD

--------VECREDNOC1004X1-------------------

ssh [soporte2@181.225.41.18](mailto:soporte2@181.225.41.18)

no interface TenGigabitEthernet0/3/0.3268

description TUNO-TOP-FOOD

bandwidth 40960

encapsulation dot1Q 3268

ip address 172.23.244.5 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.250.152 255.255.255.252 172.23.244.6 name RED1-VL3268-TUNO-TOP-FOOD

interface TenGigabitEthernet0/1/0.1823

description TOP-FOOD;ID:

bandwidth 40960

encapsulation dot1Q 1823

ip address 172.23.244.5 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.250.152 255.255.255.252 172.23.244.6 name GPON-VL1823-TUNO-TOP-FOOD

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-TOP-FOOD vlan-id 1823

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-TOP-FOOD

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-TOP-FOOD

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1823

name TUNO-TOP-FOOD

interface po4

switchport trunk allowed vlan add 1823

########################################

1824 3269 TUNO-QUINTA-EL-MAISS

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3269

description QUINTA-EL-MAISSANCO;ID:26254

bandwidth 51200

encapsulation dot1Q 3269

ip address 172.23.244.141 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.250.176 255.255.255.252 172.23.244.142 name RED1-VL3269-TUNO-QUINTA-EL-MAISSANCO

interface TenGigabitEthernet0/1/0.1824

description QUINTA-EL-MAISS;ID:26254

bandwidth 51200

encapsulation dot1Q 1824

ip address 172.23.244.141 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.250.176 255.255.255.252 172.23.244.142 name GPON-VL1824-TUNO-QUINTA-EL-MAISS

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-QUINTA-EL-MAISS vlan-id 1824

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-QUINTA-EL-MAISS

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-QUINTA-EL-MAISS

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1824

name TUNO-QUINTA-EL-MAISS

interface po4

switchport trunk allowed vlan add 1824

########################################

1825 3270 TUNO-COELLO-CVA-MER

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3270

description COELLO-CVA-MER;ID:26329

bandwidth 40960

encapsulation dot1Q 3270

ip address 172.23.244.157 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.245.232 255.255.255.248 172.23.244.158 name GPON-VL3270-TUNO-COELLO-CVA-MER

interface TenGigabitEthernet0/1/0.1825

description COELLO-CVA-MER;ID:26329

bandwidth 40960

encapsulation dot1Q 1825

ip address 172.23.244.157 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.245.232 255.255.255.248 172.23.244.158 name GPON-VL1825-TUNO-COELLO-CVA-MER

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-COELLO-CVA-MER vlan-id 1825

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-COELLO-CVA-MER

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-COELLO-CVA-MER

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1825

name TUNO-COELLO-CVA-MER

interface po4

switchport trunk allowed vlan add 1825

########################################

1826 3271 TUNO-DEST-CARUPANO

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3271

description DEST-CARUPANO;ID:26284

bandwidth 40960

encapsulation dot1Q 3271

ip address 172.23.244.173 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.253.220 255.255.255.252 172.23.244.174 name RED1-VL3271-TUNO-DEST-CARUPANO

interface TenGigabitEthernet0/1/0.1826

description DEST-CARUPANO;ID:26284

bandwidth 40960

encapsulation dot1Q 1826

ip address 172.23.244.173 255.255.255.252

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.253.220 255.255.255.252 172.23.244.174 name GPON-VL1826-TUNO-DEST-CARUPANO

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-DEST-CARUPANO vlan-id 1826

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-DEST-CARUPANO

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-DEST-CARUPANO

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1826

name TUNO-DEST-CARUPANO

interface po4

switchport trunk allowed vlan add 1826

########################################

|  |  |  |
| --- | --- | --- |
| 1827 | 3272 | TUNO-YEET-DE-VEN |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3272

description TUNO-YEET-DE-VEN

bandwidth 81920

encapsulation dot1Q 3272

ip address 172.23.243.201 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.199.200 255.255.255.252 172.23.243.202 name RED1-VL3272-TUNO-YEET-DE-VEN

interface TenGigabitEthernet0/1/0.1827

description YEET-DE-VEN;ID:

bandwidth 81920

encapsulation dot1Q 1827

ip address 172.23.243.201 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.199.200 255.255.255.252 172.23.243.202 name GPON-VL1827-TUNO-YEET-DE-VEN

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-YEET-DE-VEN vlan-id 1827

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-YEET-DE-VEN

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-YEET-DE-VEN

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1827

name TUNO-YEET-DE-VEN

interface po4

switchport trunk allowed vlan add 1827

########################################

|  |  |  |
| --- | --- | --- |
| 1828 | 3273 | TUNO-DANCINGDOLLY |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3273

description DANCINGDOLLY;ID:26637

bandwidth 30720

encapsulation dot1Q 3273

ip address 172.23.251.61 255.255.255.252

service-policy input 30M

service-policy output 30M

exit

ip route 181.225.42.96 255.255.255.248 172.23.251.62 name GPON-VL3273-TUNO-DANCINGDOLLY

interface TenGigabitEthernet0/1/0.1828

description DANCINGDOLLY;ID:26637

bandwidth 30720

encapsulation dot1Q 1828

ip address 172.23.251.61 255.255.255.252

service-policy input 30M

service-policy output 30M

exit

ip route 181.225.42.96 255.255.255.248 172.23.251.62 name GPON-VL1828-TUNO-DANCINGDOLLY

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-DANCINGDOLLY vlan-id 1828

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-DANCINGDOLLY

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-DANCINGDOLLY

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1828

name TUNO-DANCINGDOLLY

interface po4

switchport trunk allowed vlan add 1828

########################################

|  |  |  |
| --- | --- | --- |
| 1829 | 3274 | TUNO-ESTIVANELI |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3274

description RED1-VL3274-TUNO-ESTIVANELI

bandwidth 51200

encapsulation dot1Q 3274

ip address 172.23.251.113 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 181.225.42.72 255.255.255.248 172.23.251.114 name RED1-VL3274-TUNO-ESTIVANELI

interface TenGigabitEthernet0/1/0.1829

description TUNO-ESTIVANELI;ID:

bandwidth 51200

encapsulation dot1Q 1829

ip address 172.23.251.113 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 181.225.42.72 255.255.255.248 172.23.251.114 name GPON-VL1829-TUNO-ESTIVANELI

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-ESTIVANELI vlan-id 1829

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-ESTIVANELI

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-ESTIVANELI

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1829

name TUNO-ESTIVANELI

interface po4

switchport trunk allowed vlan add 1829

########################################

|  |  |  |
| --- | --- | --- |
| 1830 | 3275 | TUNO-TOLONET-FIB |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3275

description RED1-VL3275-TUNO-TOLONET-FIBRA

bandwidth 51200

encapsulation dot1Q 3275

ip address 172.23.252.93 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 181.225.40.64 255.255.255.252 172.23.252.94 name RED1-VL3275-TUNO-TOLONET

interface TenGigabitEthernet0/1/0.1830

description TOLONET-FIB;ID:

bandwidth 51200

encapsulation dot1Q 1830

ip address 172.23.252.93 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 181.225.40.64 255.255.255.252 172.23.252.94 name GPON-VL1830-TUNO-TOLONET-FIB

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-TOLONET-FIB vlan-id 1830

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-TOLONET-FIB

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-TOLONET-FIB

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1830

name TUNO-TOLONET-FIB

interface po4

switchport trunk allowed vlan add 1830

########################################

|  |  |  |
| --- | --- | --- |
| 1831 | 3276 | TUNO-PASEO-L-M |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3276

description RED1-VL3276-TUNO-PASEO-L-M

bandwidth 51200

encapsulation dot1Q 3276

ip address 172.23.250.181 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.210.88 255.255.255.252 172.23.250.182 name RED1-VL3276-TUNO-PASEO-L-M

interface TenGigabitEthernet0/1/0.1831

description TUNO-PASEO-L-M;ID:

bandwidth 51200

encapsulation dot1Q 1831

ip address 172.23.250.181 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.210.88 255.255.255.252 172.23.250.182 name GPON-VL1831-TUNO-PASEO-L-M

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-PASEO-L-M vlan-id 1831

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-PASEO-L-M

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-PASEO-L-M

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1831

name TUNO-PASEO-L-M

interface po4

switchport trunk allowed vlan add 1831

########################################

|  |  |  |
| --- | --- | --- |
| 1832 | 3277 | TUNO-EMB-RUSIA |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3277

description RED1-VL3277-TUNO-EMB-RUSIA

bandwidth 71680

encapsulation dot1Q 3277

ip address 172.23.250.229 255.255.255.252

service-policy input 70M

service-policy output 70M

exit

ip route 190.94.253.116 255.255.255.252 172.23.250.230 name RED1-VL3277-TUNO-EMB-RUSIA

ip route 190.94.253.76 255.255.255.252 172.23.250.230 name RED1-VL3277-TUNO-EMB-RUSIA

ip route 190.94.209.64 255.255.255.248 172.23.250.230 name RED1-VL3277-TUNO-EMB-RUSIA

interface TenGigabitEthernet0/1/0.1832

description EMB-RUSIA;ID:

bandwidth 71680

encapsulation dot1Q 1832

ip address 172.23.250.229 255.255.255.252

service-policy input 70M

service-policy output 70M

exit

ip route 190.94.253.116 255.255.255.252 172.23.250.230 name GPON-VL1832-TUNO-EMB-RUSIA

ip route 190.94.253.76 255.255.255.252 172.23.250.230 name GPON-VL1832-TUNO-EMB-RUSIA

ip route 190.94.209.64 255.255.255.248 172.23.250.230 name GPON-VL1832-TUNO-EMB-RUSIA

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-EMB-RUSIA vlan-id 1832

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-EMB-RUSIA

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-EMB-RUSIA

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1832

name TUNO-EMB-RUSIA

interface po4

switchport trunk allowed vlan add 1832

########################################

|  |  |  |
| --- | --- | --- |
| 1833 | 3278 | TUNO-LOBBY-AH |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3278

description RED1-VL3278-TUNO-LOBBY-AH

bandwidth 51200

encapsulation dot1Q 3278

ip address 172.23.248.1 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.210.60 255.255.255.252 172.23.248.2 name GPON-VL3283-TUNO-CONAVEN

interface TenGigabitEthernet0/1/0.1833

description LOBBY-AH;ID:

bandwidth 51200

encapsulation dot1Q 1833

ip address 172.23.248.1 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.210.60 255.255.255.252 172.23.248.2 name GPON-VL1833-TUNO-LOBBY-AH

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-LOBBY-AH vlan-id 1833

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-LOBBY-AH

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-LOBBY-AH

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1833

name TUNO- LOBBY-AH

interface po4

switchport trunk allowed vlan add 1833

########################################

|  |  |  |
| --- | --- | --- |
| 1834 | 3279 | TUNO-QTA-MARY |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3279

description RED1-VL3279-TUNO-QTA-MARY

bandwidth 51200

encapsulation dot1Q 3279

ip address 172.23.248.77 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.253.196 255.255.255.252 172.23.248.78 name RED1-VL3279-TUNO-QTA-MARY

interface TenGigabitEthernet0/1/0.1834

description QTA-MARY;ID:

bandwidth 51200

encapsulation dot1Q 1834

ip address 172.23.248.77 255.255.255.252

service-policy input 50M

service-policy output 50M

exit

ip route 190.94.253.196 255.255.255.252 172.23.248.78 name GPON-VL1834-TUNO-QTA-MARY

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-QTA-MARY vlan-id 1834

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-QTA-MARY

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-QTA-MARY

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1834

name TUNO-QTA-MARY

interface po4

switchport trunk allowed vlan add 1834

########################################

|  |  |  |
| --- | --- | --- |
| 1835 | 3280 | TUNO-FINAL-CURVE |

--------VECREDNOC1004X1-------------------

ssh soporte2@181.225.41.18

no interface TenGigabitEthernet0/3/0.3280

description FINAL-CURVE;ID:26080

bandwidth 40960

encapsulation dot1Q 3280

ip address 172.23.248.65 255.255.255.252

ip mtu 1500

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.245.168 255.255.255.248 172.23.248.66 name RED1-VL3280-TUNO-FINAL-CURVE

interface TenGigabitEthernet0/1/0.1835

description FINAL-CURVE;ID:26080

bandwidth 40960

encapsulation dot1Q 1835

ip address 172.23.248.65 255.255.255.252

ip mtu 1500

service-policy input 40M

service-policy output 40M

exit

ip route 190.94.245.168 255.255.255.248 172.23.248.66 name GPON-VL1835-TUNO-FINAL-CURVE

----------------CCSJ4500CREX2------------

ssh soporte2@172.23.253.59

set vlan TUNO-FINAL-CURVE vlan-id 1835

set interfaces ae13 unit 0 family ethernet-switching vlan members TUNO-FINAL-CURVE

set interfaces xe-0/0/14 unit 0 family ethernet-switching vlan members TUNO-FINAL-CURVE

----------------CCSC4500TUNOX1------------

ssh soporte2@172.23.253.20

vlan 1835

name TUNO-FINAL-CURVE

interface po4

switchport trunk allowed vlan add 1835